
**DECLARATION OF PERFORMANCE**

**Bond It Self Levelling Compounds**

**DOP: BDH100/ 102/103/ 105**

**EN13813:2002**

**Cementitious screed material for use internally in buildings**

**Attestation Level 4**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Levelmaster** | **Levelmaster Ad Floor** | **Levelmaster Ad Floor Plus** |
| Compressive Strength | C16 | C35 | C25 |
| Flexural Strength | F4 | F10 | F6 |
| Water Permeability | NPD | NPD | NPD |
| Water Vapour Permeability | NPD | NPD | NPD |
| Wear Resistance | NPD | NPD | NPD |
| Sound Insulation | NPD | NPD | NPD |
| Sound Absorption | NPD | NPD | NPD |
| Thermal Resistance | NPD | NPD | NPD |
| Chemical Resistance | NPD | NPD | NPD |
| Reaction To Fire | Class A1 | Class F | Class F |
| Release of Corrosive Substances | CT | CT | CT |

****

Kayleigh Cox-Nowak

Technical Manager

3rd July 2018

Seal It Services

Trading as Bond It

Unit G16 River Bank Way,

Lowfields Business Park

Elland, West Yorkshire

HX5 9DN

United Kingdom